(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "MIKROE-4319" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 19.05 7.62 0))
    (property "Value" "MIKROE-4319" (at 19.05 5.08 0))
    (property "Footprint" "MIKROE4319" (at 19.05 -94.92 0))
    (property "Datasheet" "https://download.mikroe.com/documents/mikrobu_socket/SOCKET%20mikroBUS%2016%20SMD.pdf" (at 19.05 -194.92 0))
    (property "ki_description" "mikroElektronika Products series Connector 16 SMD" (at 19.05 -294.92 0))
    (property "Height" "11.25" (at 19.05 -394.92 0))
    (property "Mouser Part Number" "932-MIKROE-4319" (at 19.05 -494.92 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mikroe/MIKROE-4319?qs=zW32dvEIR3ti011gi8UcOA%3D%3D" (at 19.05 -594.92 0))
    (property "Manufacturer_Name" "Mikroe" (at 19.05 -694.92 0))
    (property "Manufacturer_Part_Number" "MIKROE-4319" (at 19.05 -794.92 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "1")
      (number "1")
    )
    (pin passive line (at 22.86 0 180) (length 5.08)
      (name "2")
      (number "2")
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "3")
      (number "3")
    )
    (pin passive line (at 22.86 -2.54 180) (length 5.08)
      (name "4")
      (number "4")
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "5")
      (number "5")
    )
    (pin passive line (at 22.86 -5.08 180) (length 5.08)
      (name "6")
      (number "6")
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "7")
      (number "7")
    )
    (pin passive line (at 22.86 -7.62 180) (length 5.08)
      (name "8")
      (number "8")
    )
    (pin passive line (at 0 -10.16 0) (length 5.08)
      (name "9")
      (number "9")
    )
    (pin passive line (at 22.86 -10.16 180) (length 5.08)
      (name "10")
      (number "10")
    )
    (pin passive line (at 0 -12.7 0) (length 5.08)
      (name "11")
      (number "11")
    )
    (pin passive line (at 22.86 -12.7 180) (length 5.08)
      (name "12")
      (number "12")
    )
    (pin passive line (at 0 -15.24 0) (length 5.08)
      (name "13")
      (number "13")
    )
    (pin passive line (at 22.86 -15.24 180) (length 5.08)
      (name "14")
      (number "14")
    )
    (pin passive line (at 0 -17.78 0) (length 5.08)
      (name "15")
      (number "15")
    )
    (pin passive line (at 22.86 -17.78 180) (length 5.08)
      (name "16")
      (number "16")
    )
  )
)
