(footprint "MODUL USB SOUNDCARD"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" ""
		(at 19.43845 -1.085 0)
		(layer "F.SilkS")
	)
	(property "Value" "MODUL USB SOUNDCARD"
		(at 19.43845 20.962 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" thru_hole oval
		(at 3 6)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "2" thru_hole oval
		(at 3 8.5001)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "3" thru_hole oval
		(at 3 10.5001)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "4" thru_hole oval
		(at 3 13)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "5" thru_hole oval
		(at 36.5001 16.5001)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "6" thru_hole oval
		(at 29.4998 16.5001)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "7" thru_hole oval
		(at 34.9999 12)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "8" thru_hole oval
		(at 29.4998 7)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "9" thru_hole oval
		(at 36.5001 7)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
	(pad "10" thru_hole oval
		(at 34.9999 2.5001)
		(size 1.524 1.524)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(thermal_bridge_angle 0)
	)
)
