(footprint MOUDLE14P-SMD-2.54-21X17.8MM (layer F.Cu) (tedit 63BE5ED5)
  (descr "")
  (fp_text reference REF** (at 9.3345 -21.7805 0) (layer F.SilkS))
  (fp_text value MOUDLE14P-SMD-2.54-21X17.8MM (at 8.89 -10.795 0) (layer F.Fab))
  (pad 7 smd roundrect (roundrect_rratio 0.5) (at 0.835 -2.88) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd roundrect (roundrect_rratio 0.5) (at 0.835 -5.42) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd roundrect (roundrect_rratio 0.5) (at 0.835 -7.96) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd roundrect (roundrect_rratio 0.5) (at 0.835 -10.5) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd roundrect (roundrect_rratio 0.5) (at 0.835 -13.04) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd roundrect (roundrect_rratio 0.5) (at 0.835 -15.58) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 1 smd roundrect (roundrect_rratio 0.5) (at 0.835 -18.12) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd roundrect (roundrect_rratio 0.5) (at 17.0 -2.88) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd roundrect (roundrect_rratio 0.5) (at 17.0 -5.42) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd roundrect (roundrect_rratio 0.5) (at 17.0 -7.96) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd roundrect (roundrect_rratio 0.5) (at 17.0 -10.5) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd roundrect (roundrect_rratio 0.5) (at 17.0 -13.04) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd roundrect (roundrect_rratio 0.5) (at 17.0 -15.58) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd roundrect (roundrect_rratio 0.5) (at 17.0 -18.12) (size 2.75 2.0) (layers F.Cu F.Mask F.Paste))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6.35 -3.175)
        (xy 12.065 -3.175)
        (xy 12.065 -0.635)
        (xy 6.35 -0.635)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 3.683 -21.082)
        (xy 5.461 -21.082)
        (xy 5.461 -18.415)
        (xy 3.683 -18.415)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 3.683 -17.018)
        (xy 5.461 -17.018)
        (xy 5.461 -14.351)
        (xy 3.683 -14.351)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.319 -17.018)
        (xy 14.097 -17.018)
        (xy 14.097 -14.351)
        (xy 12.319 -14.351)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.319 -21.082)
        (xy 14.097 -21.082)
        (xy 14.097 -18.415)
        (xy 12.319 -18.415)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.9845 -12.7635)
        (xy 5.9055 -12.7635)
        (xy 5.9055 -10.7315)
        (xy 2.9845 -10.7315)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9.779 -11.303)
        (xy 12.827 -11.303)
        (xy 12.827 -8.255)
        (xy 9.779 -8.255)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6.35 -20.32)
        (xy 11.557 -20.32)
        (xy 11.557 -13.335)
        (xy 6.35 -13.335)
      )
    )
  )
)