(module MP1584EN-LF-P (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOIC8E_MPS_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.05in/1.27mm" (at -5.77215 -1.27) (layer Cmts.User))
  (fp_text user "0.022in/0.559mm" (at 5.77215 -1.905) (layer Cmts.User))
  (fp_text user "0.214in/5.448mm" (at 0 -4.9149) (layer Cmts.User))
  (fp_text user "0.058in/1.46mm" (at -2.72415 4.9149) (layer Cmts.User))
  (fp_text user "0.136in/3.454mm" (at 7.5819 0) (layer Cmts.User))
  (fp_text user "0.101in/2.565mm" (at 0 6.1849) (layer Cmts.User))
  (fp_text user "*" (at -2.97815 -3.6068) (layer F.SilkS))
  (fp_text user "*" (at -1.6129 -2.4257) (layer F.Fab))
  (pad 1 smd rect (at -2.72415 -1.905) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.72415 -0.635) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.72415 0.635) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.72415 1.905) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.72415 1.905) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.72415 0.635) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.72415 -0.635) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.72415 -1.905) (size 1.4605 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad EPAD smd rect (at 0 0) (size 2.5654 3.4544) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)