(module MP1720DQ-9-LF-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN10_MP1720_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.4958 -0.75) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at 4.4958 -1) (layer Cmts.User))
  (fp_text user "0.114in/2.896mm" (at 0 -3.9624) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at -1.4478 3.3274) (layer Cmts.User))
  (fp_text user "0.098in/2.5mm" (at 3.9624 0) (layer Cmts.User))
  (fp_text user "0.067in/1.7mm" (at 0 4.5974) (layer Cmts.User))
  (pad 1 smd rect (at -1.4478 -1.000001) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.4478 -0.499999) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.4478 0) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.4478 0.499999) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.4478 1.000001) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.4478 1.000001) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.4478 0.499999) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.4478 0) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.4478 -0.499999) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.4478 -1.000001) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 0) (size 1.7 2.5) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)