(module MP1921HR-A-LF-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN10_MP1921A_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.031in/0.8mm" (at -5.0165 -1.199999) (layer Cmts.User))
  (fp_text user "0.012in/0.305mm" (at 5.0165 -1.599999) (layer Cmts.User))
  (fp_text user "0.155in/3.937mm" (at 0 -4.4577) (layer Cmts.User))
  (fp_text user "0.03in/0.762mm" (at -1.9685 3.8227) (layer Cmts.User))
  (fp_text user "0.118in/3mm" (at 4.4577 0) (layer Cmts.User))
  (fp_text user "0.102in/2.6mm" (at 0 5.0927) (layer Cmts.User))
  (pad 1 smd rect (at -1.9685 -1.599999) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.9685 -0.799998) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.9685 0) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.9685 0.800001) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.9685 1.599999) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.9685 1.599999) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.9685 0.799998) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.9685 0) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.9685 -0.800001) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.9685 -1.599999) (size 0.762 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 0) (size 2.6 2.999999) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)