(module MP1922GV-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-22_MP1922_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at 0 5.4737) (layer Cmts.User))
  (fp_text user "0.151in/3.835mm" (at 0 8.1407) (layer Cmts.User))
  (fp_text user "0.191in/4.851mm" (at 9.9187 0) (layer Cmts.User))
  (fp_text user "0.034in/0.864mm" (at 2.4257 -4.9657) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -3.8227 -1.25) (layer Cmts.User))
  (fp_text user "*" (at -3.1369 -1.25) (layer F.SilkS))
  (fp_text user "*" (at -0.6985 -1.25) (layer F.Fab))
  (pad 1 smd rect (at -1.9177 -1.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.9177 -0.750001 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.9177 -0.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.9177 0.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.9177 0.750001 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.9177 1.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.000001 2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -0.499999 2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.499999 2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.000001 2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.9177 1.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.9177 0.750001 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.9177 0.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 1.9177 -0.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 1.9177 -0.750001 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 1.9177 -1.25 90) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 1.000001 -2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 0.499999 -2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 0 -2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -0.499999 -2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at -1.000001 -2.4257) (size 0.254 0.8636) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 0 0) (size 2.4 1.8) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)