(module MP2192GC-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value WLCSP-6_MP2192_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "A" (at -1.0795 -0.4) (layer F.SilkS))
  (fp_text user "A" (at -1.0795 -0.4) (layer F.Fab))
  (fp_text user "A" (at -1.0795 -0.4) (layer B.SilkS))
  (fp_text user "C" (at -1.0795 0.4) (layer F.SilkS))
  (fp_text user "C" (at -1.0795 0.4) (layer F.Fab))
  (fp_text user "C" (at -1.0795 0.4) (layer B.SilkS))
  (fp_text user "1" (at -0.2 -1.2827 90) (layer F.SilkS))
  (fp_text user "1" (at -0.2 -1.2827 90) (layer F.Fab))
  (fp_text user "1" (at -0.2 -1.2827 90) (layer B.SilkS))
  (fp_text user "2" (at 0.2 -1.2827 90) (layer F.SilkS))
  (fp_text user "2" (at 0.2 -1.2827 90) (layer F.Fab))
  (fp_text user "2" (at 0.2 -1.2827 90) (layer B.SilkS))
  (fp_text user "0.2in/5.08mm" (at 2.8575 0) (layer Cmts.User))
  (fp_text user "0.15in/3.81mm" (at 0 3.0607) (layer Cmts.User))
  (fp_text user "0.016in/0.4mm" (at 2.8575 -0.2) (layer Cmts.User))
  (fp_text user "0.009in/0.229mm" (at 2.8575 0.4) (layer Cmts.User))
  (pad A1 smd circle (at -0.2 -0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0.2 -0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at -0.2 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd circle (at 0.2 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad C1 smd circle (at -0.2 0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad C2 smd circle (at 0.2 0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)