(module MP2332HGTL-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOT583_MP2332H_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -3.7973 -0.5) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at 3.7973 -0.246) (layer Cmts.User))
  (fp_text user "0.011in/0.279mm" (at 3.7973 -0.75) (layer Cmts.User))
  (fp_text user "0.059in/1.499mm" (at 0 -3.5179) (layer Cmts.User))
  (fp_text user "0.024in/0.61mm" (at -0.7493 2.8829) (layer Cmts.User))
  (pad 1 smd rect (at -0.7493 -0.750001) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.7493 -0.25) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.7493 0.25) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.7493 0.750001) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.7493 0.750001) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.7493 0.25) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.7493 -0.25) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.7493 -0.750001) (size 0.6096 0.2794) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)