(module MP2602DQ-LF-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-3x3_MP2602_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.853599 0.25) (layer Cmts.User))
  (fp_text user "0.114in/2.9mm" (at 0 5.9436) (layer Cmts.User))
  (fp_text user "0in/0mm" (at 9.2224 0) (layer Cmts.User))
  (fp_text user "0.028in/0.711mm" (at 0 -4.497999) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -7.3936 -1) (layer Cmts.User))
  (fp_text user "0.067in/1.702mm" (at 0 3.4036) (layer Cmts.User))
  (fp_text user "0.098in/2.489mm" (at 4.142399 0) (layer Cmts.User))
  (pad 1 smd rect (at -1.45 -1.000001) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.45 -0.499999) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.45 0) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.45 0.499999) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.45 1.000001) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.45 1.000001) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.45 0.499999) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.45 0) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.45 -0.499999) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.45 -1.000001) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 0) (size 1.7018 2.4892) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)