(module MP26123DR-LF-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN16_MP26123_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at 0 4.8895) (layer Cmts.User))
  (fp_text user "0.145in/3.683mm" (at 0 7.5819) (layer Cmts.User))
  (fp_text user "0.145in/3.683mm" (at 9.8171 0) (layer Cmts.User))
  (fp_text user "0.04in/1.016mm" (at 1.8415 -4.8895) (layer Cmts.User))
  (fp_text user "0.012in/0.305mm" (at -3.7719 -0.975) (layer Cmts.User))
  (fp_text user "*" (at -3.1369 -0.975) (layer F.SilkS))
  (fp_text user "*" (at -0.5461 -0.975) (layer F.Fab))
  (pad 1 smd rect (at -1.8415 -0.974999 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.8415 -0.325001 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.8415 0.325001 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.8415 0.974999 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.974999 1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -0.325001 1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.325001 1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.974999 1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.8415 0.974999 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.8415 0.325001 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.8415 -0.325001 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.8415 -0.974999 90) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0.974999 -1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 0.325001 -1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -0.325001 -1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -0.974999 -1.8415) (size 0.3048 1.016) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 0 0) (size 2.3114 2.3114) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)