(module MP2639BGR-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-4x4_MP2639B_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.016in/0.4mm" (at -5.5372 0.2) (layer Cmts.User))
  (fp_text user "0.125in/3.175mm" (at 0 8.4397) (layer Cmts.User))
  (fp_text user "0.154in/3.9mm" (at 8.8138 0) (layer Cmts.User))
  (fp_text user "0.071in/1.803mm" (at 1.95 -4.6355) (layer Cmts.User))
  (fp_text user "0.012in/0.305mm" (at -8.0772 -1.2) (layer Cmts.User))
  (pad 1 smd rect (at -1.3995 -1.100001) (size 1.8034 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.3995 -0.549999) (size 1.8034 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.3995 0) (size 1.8034 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.3995 0.549999) (size 1.8034 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.3995 1.100001) (size 1.8034 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.3 1.950001 90) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -0.800001 1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -0.399999 1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.399999 1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0.800001 1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.3 1.950001 90) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.7755 1.2) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.7755 0.800001) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 1.7755 0.399999) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 1.7755 0) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 1.7755 -0.399999) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 1.7755 -0.800001) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 1.7755 -1.2) (size 1.0414 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 1.3 -1.950001 90) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 0.800001 -1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 0.399999 -1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 0 -1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at -0.399999 -1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at -0.800001 -1.950001 90) (size 0.7112 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at -1.3 -1.950001 90) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)