(module MP2662 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value WLCSP-9_1p75MMx1p75MM_MP2662_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "A" (at -1.5367 -0.5) (layer F.SilkS))
  (fp_text user "A" (at -1.5367 -0.5) (layer F.Fab))
  (fp_text user "A" (at -1.5367 -0.5) (layer B.SilkS))
  (fp_text user "C" (at -1.5367 0.5) (layer F.SilkS))
  (fp_text user "C" (at -1.5367 0.5) (layer F.Fab))
  (fp_text user "C" (at -1.5367 0.5) (layer B.SilkS))
  (fp_text user "1" (at -0.5 -1.5367 90) (layer F.SilkS))
  (fp_text user "1" (at -0.5 -1.5367 90) (layer F.Fab))
  (fp_text user "1" (at -0.5 -1.5367 90) (layer B.SilkS))
  (fp_text user "3" (at 0.5 -1.5367 90) (layer F.SilkS))
  (fp_text user "3" (at 0.5 -1.5367 90) (layer F.Fab))
  (fp_text user "3" (at 0.5 -1.5367 90) (layer B.SilkS))
  (fp_text user "0.2in/5.08mm" (at 3.3147 0) (layer Cmts.User))
  (fp_text user "0.15in/3.81mm" (at 0 3.3147) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at 3.3147 -0.25) (layer Cmts.User))
  (fp_text user "0.011in/0.279mm" (at 3.3147 0.5) (layer Cmts.User))
  (pad A1 smd circle (at -0.5 -0.5) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0 -0.5) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd circle (at 0.5 -0.5) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at -0.5 0) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd circle (at 0 0) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd circle (at 0.5 0) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad C1 smd circle (at -0.5 0.5) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad C2 smd circle (at 0 0.5) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad C3 smd circle (at 0.5 0.5) (size 0.2794 0.2794) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)