(module MP2667 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-10_2MMx2MM_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -2.9845 -0.5) (layer Cmts.User))
  (fp_text user "0.028in/0.711mm" (at -1.0033 -4.0513) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -4.0513 1.0033) (layer Cmts.User))
  (fp_text user "0.079in/2.007mm" (at 0 6.5913) (layer Cmts.User))
  (fp_text user "0.079in/2.007mm" (at 6.5913 0.635) (layer Cmts.User))
  (fp_text user "*" (at -1.9939 -1) (layer F.SilkS))
  (fp_text user "*" (at -0.6477 -1) (layer F.Fab))
  (pad 1 smd rect (at -1.0033 -0.750001 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.0033 -0.25 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.0033 0.25 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.0033 0.750001 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 1.0033) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.0033 0.750001 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.0033 0.25 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.0033 -0.25 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.0033 -0.750001 90) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0 -1.0033) (size 0.254 0.7112) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)