(module MP28160GC-P (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value WLCSP-1p4x1p8_MP28160_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "A" (at -1.3589 -0.6) (layer F.SilkS))
  (fp_text user "A" (at -1.3589 -0.6) (layer F.Fab))
  (fp_text user "A" (at -1.3589 -0.6) (layer B.SilkS))
  (fp_text user "D" (at -1.3589 0.6) (layer F.SilkS))
  (fp_text user "D" (at -1.3589 0.6) (layer F.Fab))
  (fp_text user "D" (at -1.3589 0.6) (layer B.SilkS))
  (fp_text user "1" (at -0.4 -1.5621 90) (layer F.SilkS))
  (fp_text user "1" (at -0.4 -1.5621 90) (layer F.Fab))
  (fp_text user "1" (at -0.4 -1.5621 90) (layer B.SilkS))
  (fp_text user "3" (at 0.4 -1.5621 90) (layer F.SilkS))
  (fp_text user "3" (at 0.4 -1.5621 90) (layer F.Fab))
  (fp_text user "3" (at 0.4 -1.5621 90) (layer B.SilkS))
  (fp_text user "0.2in/5.08mm" (at 3.1369 0) (layer Cmts.User))
  (fp_text user "0.15in/3.81mm" (at 0 3.3401) (layer Cmts.User))
  (fp_text user "0.016in/0.4mm" (at 3.1369 -0.4) (layer Cmts.User))
  (fp_text user "0.009in/0.229mm" (at 3.1369 0.6) (layer Cmts.User))
  (pad A1 smd circle (at -0.4 -0.6) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad A2 smd circle (at 0 -0.6) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad A3 smd circle (at 0.4 -0.6) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad B1 smd circle (at -0.4 -0.2) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad B2 smd circle (at 0 -0.2) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad B3 smd circle (at 0.4 -0.2) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad C1 smd circle (at -0.4 0.2) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad C2 smd circle (at 0 0.2) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad C3 smd circle (at 0.4 0.2) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad D1 smd circle (at -0.4 0.6) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad D2 smd circle (at 0 0.6) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad D3 smd circle (at 0.4 0.6) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)