(module MP3432GL-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-3x4_MP3432_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.5974 0.25) (layer Cmts.User))
  (fp_text user "0.051in/1.3mm" (at 0 7.8944) (layer Cmts.User))
  (fp_text user "0.15in/3.8mm" (at 8.3716 0) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at 1.9 -3.698) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -6.6444 -0.5) (layer Cmts.User))
  (pad 1 smd rect (at -0.649999 0) (size 2.3114 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.000001 1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.499999 1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0 1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.499999 1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.000001 1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.649999 0.599999) (size 2.3114 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.649999 -0.599999) (size 2.3114 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.000001 -1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.499999 -1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 -1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.499999 -1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -1.000001 -1.899999 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)