(module MP4572GQB-P (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-12_MP4572_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.028in/0.7mm" (at 1 -4.048) (layer Cmts.User))
  (fp_text user "0.01in/0.25mm" (at -6.938 -0.250063) (layer Cmts.User))
  (fp_text user "0.079in/2mm" (at 0 7.387999) (layer Cmts.User))
  (fp_text user "0.114in/2.9mm" (at 8.778 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.398 0) (layer Cmts.User))
  (fp_text user "*" (at -1.985 -0.375063) (layer F.SilkS))
  (fp_text user "*" (at -0.215 -0.375063) (layer F.Fab))
  (pad 1 smd rect (at -1.100001 -0.375063) (size 0.9 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.000001 0.375063) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.750189 1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.250063 1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.250063 1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.750189 1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.000001 0.425063) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.000001 -0.425063) (size 1.1 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.750189 -1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.250063 -1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -0.250063 -1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.750189 -1.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)