(module MP5035GJ-P (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value TSOT23-6_MP5035_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.037in/0.95mm" (at -4.40055 -0.475) (layer Cmts.User))
  (fp_text user "0.022in/0.559mm" (at 4.40055 -0.95) (layer Cmts.User))
  (fp_text user "0.106in/2.705mm" (at 0 -3.9116) (layer Cmts.User))
  (fp_text user "0.04in/1.003mm" (at -1.35255 3.9116) (layer Cmts.User))
  (fp_text user "*" (at -1.60655 -2.6518) (layer F.SilkS))
  (fp_text user "*" (at -0.4699 -1.4224) (layer F.Fab))
  (pad 1 smd rect (at -1.35255 -0.950001) (size 1.0033 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.35255 0) (size 1.0033 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.35255 0.950001) (size 1.0033 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.35255 0.950001) (size 1.0033 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.35255 0) (size 1.0033 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.35255 -0.950001) (size 1.0033 0.5588) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)