(module MP5098GDT-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value TQFN-10_MP5098_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.028in/0.7mm" (at 0.95 -3.998) (layer Cmts.User))
  (fp_text user "0.006in/0.15mm" (at -6.888 -0.35) (layer Cmts.User))
  (fp_text user "0.014in/0.35mm" (at -4.348 0.175) (layer Cmts.User))
  (fp_text user "0.075in/1.9mm" (at 0 7.387999) (layer Cmts.User))
  (fp_text user "0.114in/2.9mm" (at 8.728 0) (layer Cmts.User))
  (fp_text user "*" (at -1.935 -0.35) (layer F.SilkS))
  (fp_text user "*" (at 0.035 -0.35) (layer F.Fab))
  (pad 1 smd rect (at -0.950001 -0.349999) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.950001 0) (size 0.7 0.15) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.950001 0.349999) (size 0.7 0.15) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.250001 1.45 90) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.250001 1.45 90) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.950001 0.349999) (size 0.7 0.15) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.950001 0) (size 0.7 0.15) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.950001 -0.349999) (size 0.7 0.15) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.250001 -1.45 90) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -0.250001 -1.45 90) (size 0.7 0.2) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)