(module MP9989GS-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOIC-8_MP9989_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.063in/1.6mm" (at -2.7 -5.5499) (layer Cmts.User))
  (fp_text user "0.05in/1.27mm" (at -5.748 -1.27) (layer Cmts.User))
  (fp_text user "0.213in/5.4mm" (at 0 4.953) (layer Cmts.User))
  (fp_text user "0.024in/0.61mm" (at 5.748 -1.905) (layer Cmts.User))
  (pad 1 smd rect (at -2.7 -1.905) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.7 -0.635) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.7 0.635) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.7 1.905) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.7 1.905) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.7 0.635) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.7 -0.635) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.7 -1.905) (size 1.6002 0.6096) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)