(module QFN-59_10MMx12MMx4MM_MPM3695-2 (layer F.Cu) (tedit 65E87319)
  (attr smd)
  (fp_text reference REF** (at -0.0962 0) (layer F.SilkS))
  (fp_text value QFN-59_10MMx12MMx4MM_MPM3695-2 (at 17.3212 0) (layer F.Fab))
  (fp_text user "Default Padstyle: RX61Y12D0T" (at -15.2035 13.0537) (layer Dwgs.User))
  (fp_text user "Heat Tab Padstyle: RX63Y79D0T" (at -16.1525 14.5777) (layer Dwgs.User))
  (fp_text user "Alt 1 Padstyle: RX49Y12D0T" (at -14.2373 17.6257) (layer Dwgs.User))
  (fp_text user "Alt 2 Padstyle: OX90Y60D30P" (at -14.8136 19.1497) (layer Dwgs.User))
  (fp_text user 0.026in/0.65mm (at -4.0793 -8.0076) (layer Dwgs.User))
  (fp_text user 0.398in/10.109mm (at -4.3305 -9.8943) (layer Dwgs.User))
  (fp_text user 0.077in/1.95mm (at -15.0062 1.2925) (layer Dwgs.User))
  (fp_text user 0.026in/0.65mm (at -15.0978 -1.3075) (layer Dwgs.User))
  (fp_text user 0.476in/12.09mm (at 8.0555 0.3175) (layer Dwgs.User))
  (pad 50 smd rect (at 1.3 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 52 smd rect (at -0.65 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 1 smd custom (at -4.525 -5.2) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.1747 -0.5004) (xy 0.4723 -0.5004) (xy 0.4726 -1.1003) (xy 0.7774 -1.1003) (xy 0.7747 -0.1524)
         (xy 0.4726 0.1443) (xy -0.7747 0.1524) (xy -0.7747 -0.1524) (xy -0.1747 -0.1524)) (width 0.0254))
    ))
  (pad 2 smd rect (at -4.525 -4.55) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 3 smd rect (at -4.525 -3.9) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 4 smd rect (at -4.525 -3.25) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 5 smd rect (at -4.525 -2.6) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 6 smd rect (at -4.525 -1.95) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 7 smd rect (at -4.525 -1.3) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 8 smd rect (at -4.525 -0.65) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 9 smd custom (at -4.525 0) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.1747 0.1524) (xy 0.7747 0.1524) (xy 0.7747 -0.1524) (xy 2.7247 -0.1524) (xy 2.7247 0.8024)
         (xy 0.7747 0.8024) (xy 0.7747 0.4976) (xy -0.1747 0.4976)) (width 0.0254))
    ))
  (pad 10 smd rect (at -4.525 0.65) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 11 smd custom (at -4.525 1.95) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 2.7247 -0.1524) (xy 2.7247 1.4324) (xy 0.7747 1.4324) (xy 0.7747 1.1276) (xy -0.1747 1.1276)
         (xy -0.1747 0.8024) (xy 0.7747 0.8024) (xy 0.7747 0.4976) (xy -0.1747 0.4976) (xy -0.1747 0.1524)
         (xy 0.7747 0.1524) (xy 0.7747 -0.1524)) (width 0.0254))
    ))
  (pad 12 smd rect (at -4.525 2.6) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 13 smd rect (at -4.525 3.23) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 14 smd rect (at -4.525 3.88) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 15 smd rect (at -4.525 4.53) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 16 smd custom (at -4.525 5.18) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.7747 -0.1524) (xy 0.7747 -0.1524) (xy 0.7774 1.1203) (xy 0.4726 1.1203) (xy 0.4723 0.5004)
         (xy -0.1747 0.5004) (xy -0.1747 0.1524) (xy -0.7747 0.1524)) (width 0.0254))
    ))
  (pad 17 smd rect (at -3.9 5.678 90) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 18 smd rect (at -3.25 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 19 smd rect (at -2.6 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 20 smd rect (at -1.95 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 21 smd rect (at -1.3 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 23 smd custom (at 0 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -0.8024 -1.9783) (xy 0.8024 -1.9783) (xy 0.8024 -0.6223) (xy 0.4976 -0.6223) (xy 0.4976 0.0223)
         (xy 0.1524 0.0223) (xy 0.1524 -0.6223) (xy -0.1524 -0.6223) (xy -0.1524 0.0223) (xy -0.4976 0.0223)
         (xy -0.4976 -0.6223) (xy -0.8024 -0.6223)) (width 0.0254))
    ))
  (pad 24 smd rect (at 0.65 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 25 smd rect (at 1.3 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 26 smd rect (at 1.95 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 27 smd rect (at 2.6 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 28 smd rect (at 3.25 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 29 smd custom (at 3.9 5.678) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 1.3997 -0.6504) (xy -0.1497 -0.6504) (xy -0.1524 0.6223) (xy 0.1524 0.6223) (xy 0.1527 0.0024)
         (xy 0.7997 0.0024) (xy 0.7997 -0.3456) (xy 1.3997 -0.3456)) (width 0.0254))
    ))
  (pad 30 smd rect (at 4.525 5.18 180) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 31 smd rect (at 4.525 4.53 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 32 smd rect (at 4.525 3.88 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 33 smd custom (at 4.525 3.23) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy -2.7247 -1.4324) (xy -2.7247 0.1524) (xy -0.7747 0.1524) (xy -0.7747 -0.1524) (xy 0.1747 -0.1524)
         (xy 0.1747 -0.4776) (xy -0.7747 -0.4776) (xy -0.7747 -0.7824) (xy 0.1747 -0.7824) (xy 0.1747 -1.1276)
         (xy -0.7747 -1.1276) (xy -0.7747 -1.4324)) (width 0.0254))
    ))
  (pad 34 smd rect (at 4.525 2.6 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 35 smd rect (at 4.525 1.95 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 36 smd custom (at 4.525 0.65) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.1747 -0.4976) (xy -0.7747 -0.4976) (xy -0.7747 -0.8024) (xy -2.7247 -0.8024) (xy -2.7247 0.1524)
         (xy -0.7747 0.1524) (xy -0.7747 -0.1524) (xy 0.1747 -0.1524)) (width 0.0254))
    ))
  (pad 37 smd rect (at 4.525 0 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 38 smd rect (at 4.525 -0.65 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 39 smd rect (at 4.525 -1.3 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 40 smd rect (at 4.525 -1.95 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 41 smd rect (at 4.525 -2.6 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 42 smd rect (at 4.525 -3.25 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 43 smd rect (at 4.525 -3.9 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 44 smd rect (at 4.525 -4.55 180) (size 1.5494 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 45 smd custom (at 4.525 -5.2) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102) (zone_connect 2)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.7747 0.1524) (xy -0.7747 0.1524) (xy -0.7774 -1.1003) (xy -0.4726 -1.1003) (xy -0.4723 -0.5004)
         (xy 0.1747 -0.5004) (xy 0.1747 -0.1524) (xy 0.7747 -0.1524)) (width 0.0254))
    ))
  (pad 46 smd rect (at 3.9 -5.678 270) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 47 smd rect (at 3.25 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 48 smd rect (at 2.6 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 49 smd rect (at 1.95 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 51 smd rect (at 0.65 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 53 smd rect (at -1.3 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 54 smd rect (at -1.95 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 55 smd rect (at -2.6 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 56 smd rect (at -3.25 -5.678 270) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 57 smd rect (at -3.9 -5.678 270) (size 0.127 0.127) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
  (pad 59 smd rect (at 0 1.697) (size 1.6002 2.0066) (layers F.Cu F.Mask)
    (solder_mask_margin 0.102))
  (pad 58 smd rect (at 0 -1.703) (size 1.6002 2.0066) (layers F.Cu F.Mask)
    (solder_mask_margin 0.102))
  (pad 22 smd rect (at -0.65 5.678 90) (size 1.2446 0.3048) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.102))
)
