(module MPM54304GMN-0004 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value LGA7x7x2_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -5.2578 -1.3) (layer Cmts.User))
  (fp_text user "0.039in/0.991mm" (at -2.9845 -6.0325) (layer Cmts.User))
  (fp_text user "0.014in/0.356mm" (at -6.0325 2.9845) (layer Cmts.User))
  (fp_text user "0.235in/5.969mm" (at 0 8.5725) (layer Cmts.User))
  (fp_text user "0.235in/5.969mm" (at 8.5725 0.635) (layer Cmts.User))
  (fp_text user "0.138in/3.505mm" (at 0 4.8006) (layer Cmts.User))
  (fp_text user "0.138in/3.505mm" (at 4.8006 -0.635) (layer Cmts.User))
  (fp_text user "*" (at -4.1148 -1.95) (layer F.SilkS))
  (fp_text user "*" (at -2.4892 -1.95) (layer F.Fab))
  (pad 1 smd rect (at -2.9845 -1.625001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.9845 -0.974999 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.9845 -0.325001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.9845 0.325001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.9845 0.974999 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.9845 1.625001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.925 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -2.274999 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.625001 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -0.974999 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -0.325001 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 0.325001 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0.974999 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.625001 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 2.274999 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 2.925 2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 2.9845 1.625001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 2.9845 0.974999 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 2.9845 0.325001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 2.9845 -0.325001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 2.9845 -0.974999 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 2.9845 -1.625001 90) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 2.925 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 2.274999 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 1.625001 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 0.974999 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 0.325001 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at -0.325001 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at -0.974999 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at -1.625001 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at -2.274999 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at -2.925 -2.9845) (size 0.3556 0.9906) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 0 0) (size 3.5052 3.5052) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)