(module MPQ4572GQBE-AEC1-Z (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-2p5x3_MPQ4572-AEC1_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.4925 0) (layer Cmts.User))
  (fp_text user "0.079in/2mm" (at 0 7.3936) (layer Cmts.User))
  (fp_text user "0.114in/2.9mm" (at 8.7724 0) (layer Cmts.User))
  (fp_text user "0.028in/0.711mm" (at 1 -4.048) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -6.9436 -0.25) (layer Cmts.User))
  (fp_text user "*" (at -2.0795 -0.25) (layer F.SilkS))
  (fp_text user "*" (at 0.0795 -0.25) (layer F.Fab))
  (pad 1 smd rect (at -1.102001 -0.375) (size 0.899998 0.250012) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.000001 0.375) (size 1.099998 0.250012) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.750001 1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.25 1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.25 1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.750001 1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.000001 0.425) (size 1.099998 0.250012) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.000001 -0.425) (size 1.099998 0.250012) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.750001 -1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 0.25 -1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -0.25 -1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.750001 -1.45 90) (size 0.7112 0.254) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)