(module MPQ6614GDE-AEC1-P (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN-8_MPQ6614-AEC1_MNP (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -3.8735 -0.65) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at 3.8735 -0.975) (layer Cmts.User))
  (fp_text user "0.065in/1.651mm" (at 0 -3.9624) (layer Cmts.User))
  (fp_text user "0.042in/1.067mm" (at -0.8255 3.3274) (layer Cmts.User))
  (pad 1 smd rect (at -0.8255 -0.974999) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.8255 -0.325001) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.8255 0.325001) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.8255 0.974999) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.8255 0.974999) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.8255 0.325001) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.8255 -0.325001) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.8255 -0.974999) (size 1.0668 0.254) (layers F.Cu F.Paste F.Mask))
  (tags "ultralibrarian")
)