(module MPRLS0300YG00001B (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value MPRLS0300YG00001B_HNW (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.05in/1.27mm" (at -4.203 -0.635) (layer Cmts.User))
  (fp_text user "0.026in/0.66mm" (at -2.0948 -5.1428) (layer Cmts.User))
  (fp_text user "0.028in/0.711mm" (at -5.1428 2.0948) (layer Cmts.User))
  (fp_text user "0.165in/4.19mm" (at 0 7.6828) (layer Cmts.User))
  (fp_text user "0.165in/4.19mm" (at 7.6828 0.635) (layer Cmts.User))
  (fp_text user "*" (at -3.06 -1.905) (layer F.SilkS))
  (fp_text user "*" (at -1.7646 -1.905) (layer F.Fab))
  (pad 3 smd rect (at -2.094802 -1.27 90) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.094802 0 90) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.094802 1.27 90) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -1.27 2.094802) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 2.094802) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.27 2.094802) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 2.094802 1.27 90) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.094802 0 90) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.094802 -1.27 90) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.27 -2.094802) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 -2.094802) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.27 -2.094802) (size 0.7112 0.6604) (layers F.Cu F.Paste F.Mask))
)
