(module Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm (layer F.Cu) (tedit 5DC5FE75)
  (descr "MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "MSOP SO")
  (attr smd)
  (fp_text reference REF** (at 0 -2.45) (layer F.SilkS))
  (fp_text value MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm (at 0 2.45) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd roundrect (at 0.42 0.47) (size 0.68 0.76) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.42 -0.47) (size 0.68 0.76) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.42 0.47) (size 0.68 0.76) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.42 -0.47) (size 0.68 0.76) (layers F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd rect (at 0 0) (size 1.68 1.88) (layers F.Cu F.Mask))
  (pad 8 smd roundrect (at 2.15 -0.975) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 2.15 -0.325) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 2.15 0.325) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 2.15 0.975) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at -2.15 0.975) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -2.15 0.325) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -2.15 -0.325) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -2.15 -0.975) (size 1.45 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
