(module ND005D-SM02-M (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value LGA-11_ND_STN (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.075in/1.91mm" (at -9.652 0) (layer Cmts.User))
  (fp_text user "0.4in/10.16mm" (at 0 15.24) (layer Cmts.User))
  (fp_text user "0.65in/16.51mm" (at 11.811 0) (layer Cmts.User))
  (fp_text user "0.11in/2.794mm" (at 5.08 -8.128) (layer Cmts.User))
  (fp_text user "0.05in/1.27mm" (at -12.065 -2.865) (layer Cmts.User))
  (fp_text user "*" (at -7.112 -2.865) (layer F.SilkS))
  (fp_text user "*" (at -3.048 -2.865) (layer F.Fab))
  (pad 7 smd rect (at -5.08 -2.670001) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -5.08 4.450001) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -5.08 6.479999) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -5.08 8.510001) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.910001 8.51 90) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 1.910001 8.51 90) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 5.08 8.510001) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 5.08 6.479999) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 5.08 4.450001) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 5.08 -2.670001) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0 -8.51 90) (size 2.794 1.27) (layers F.Cu F.Paste F.Mask))
)
