(module NX2012SA-32.768KHZ-EXS00A-MU00389 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value XTAL_NX2012SA_NDK (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.049in/1.245mm" (at 3.7592 0) (layer Cmts.User))
  (fp_text user "0.018in/0.457mm" (at -0.7112 2.4003) (layer Cmts.User))
  (pad 1 smd rect (at -0.7112 0) (size 0.4572 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.7112 0) (size 0.4572 1.2446) (layers F.Cu F.Paste F.Mask))
)
