(footprint "NX2016SA_NDK" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "NX2016SA-32MHZ-EXS00A-CS06654 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value NX2016SA_NDK (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" smd rect (at -0.525 -0.675) (size 0.762 0.8382) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -0.525 0.675) (size 0.762 0.8382) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 0.525 0.675) (size 0.762 0.8382) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 0.525 -0.675) (size 0.762 0.8382) (layers "F.Cu" "F.Paste" "F.Mask"))
)
