(module NX3225GD-8MHZ-STD-CRA-3 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value XTAL_NX3225GD-8MHZ-STD-CRA-3_NDK (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.094in/2.388mm" (at 4.0005 0) (layer Cmts.User))
  (fp_text user "0.051in/1.295mm" (at -0.9525 3.0734) (layer Cmts.User))
  (pad 1 smd rect (at -0.9525 0) (size 1.2954 2.3876) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.9525 0) (size 1.2954 2.3876) (layers F.Cu F.Paste F.Mask))
)
