(module NX3225SA-12MHZ-STD-CSR-6 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value NX3225SA_NDK (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.063in/1.6mm" (at -1.778 1.6002) (layer Cmts.User))
  (fp_text user "0.051in/1.295mm" (at 0.4953 -4.3561) (layer Cmts.User))
  (fp_text user "0.033in/0.838mm" (at -2.5527 1.3081) (layer Cmts.User))
  (fp_text user "-0.039in/-0.991mm" (at 0 6.8961) (layer Cmts.User))
  (fp_text user "0.103in/2.616mm" (at 5.0927 0.635) (layer Cmts.User))
  (fp_text user "*" (at -0.8001 -2.5908) (layer F.SilkS))
  (fp_text user "*" (at -0.8001 -0.6604) (layer F.Fab))
  (pad 1 smd rect (at -0.8001 -1.3081) (size 0.8382 1.2954) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.8001 1.3081) (size 0.8382 1.2954) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.8001 1.3081) (size 0.8382 1.2954) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.8001 -1.3081) (size 0.8382 1.2954) (layers F.Cu F.Paste F.Mask))
)
