(module OnSemi_CASE100CY (layer F.Cu) (tedit 5B870A92)
  (descr "OnSemi CASE 100CY, light-direction upwards, see http://www.onsemi.com/pub/Collateral/QRE1113-D.PDF")
  (tags "refective opto couple photo coupler")
  (attr smd)
  (fp_text reference REF** (at -2.5 0 90) (layer F.SilkS))
  (fp_text value OnSemi_CASE100CY (at 0 3.9) (layer F.Fab))
  (fp_text user %R (at 0 0.2) (layer F.Fab))
  (pad 3 smd rect (at 0.9 2) (size 0.79 1.66) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.9 2) (size 0.79 1.66) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.9 -2) (size 0.79 1.66) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.9 -2) (size 0.79 1.66) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/OptoDevice.3dshapes/OnSemi_CASE100CY.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
