(footprint "Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "SMD Crystal Oscillator IDT https://www.idt.com/document/dst/xu-family-datasheet#page=15, 5.0x3.2mm")
	(tags "SMD SMT crystal oscillator")
	(property "Reference" "REF**"
		(at 0 -3.61 0)
		(layer "F.SilkS")
	)
	(property "Value" "Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm"
		(at 0 3.67 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.125 -1.27 270)
		(size 0.89 1.29)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -1.125 0 270)
		(size 0.89 1.29)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -1.125 1.27 270)
		(size 0.89 1.29)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at 1.125 1.27 270)
		(size 0.89 1.29)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at 1.125 0 270)
		(size 0.89 1.29)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 1.125 -1.27 270)
		(size 0.89 1.29)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_IDT_JS6-6_5.0x3.2mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)