(module PC81710NIP1B (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOP_PC8171_SCT (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -7.4041 0) (layer Cmts.User))
  (fp_text user "0.057in/1.448mm" (at 7.4041 -1.27) (layer Cmts.User))
  (fp_text user "0.343in/8.712mm" (at 0 -4.8895) (layer Cmts.User))
  (fp_text user "0.079in/2.007mm" (at -4.3561 4.8895) (layer Cmts.User))
  (fp_text user "*" (at -4.6101 -3.8608) (layer F.SilkS))
  (fp_text user "*" (at -3.1242 -2.4003) (layer F.Fab))
  (pad 1 smd rect (at -4.3561 -1.27) (size 2.0066 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -4.3561 1.27) (size 2.0066 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 4.3561 1.27) (size 2.0066 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 4.3561 -1.27) (size 2.0066 1.4478) (layers F.Cu F.Paste F.Mask))
)
