(module PESD5V0X1BCSFYL (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value RELAY_PESD5V0X1BCSF_NEX (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at 3.2512 0) (layer Cmts.User))
  (fp_text user "0.006in/0.152mm" (at -0.2032 1.9431) (layer Cmts.User))
  (pad 1 smd rect (at -0.2032 0) (size 0.1524 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.2032 0) (size 0.1524 0.254) (layers F.Cu F.Paste F.Mask))
)
