(module PIC18F26K80-H&slash_MM (layer F.Cu) (tedit 65B14CCB)
  (fp_text reference REF** (at 0 -4.65) (layer F.SilkS))
  (fp_text value QFN-S28_6x6MC_MCH (at 0 4.8) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user * (at -3.937 -2.275) (layer F.SilkS))
  (fp_text user * (at -2.4892 -2.275) (layer F.Fab))
  (pad 1 smd rect (at -2.8956 -1.950001 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.8956 -1.3 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.8956 -0.649999 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.8956 0 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.8956 0.649999 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.8956 1.3 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.8956 1.949999 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.950001 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.3 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -0.650001 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 0.649999 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.3 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.949999 2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 2.8956 1.950001 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 2.8956 1.3 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 2.8956 0.650001 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 2.8956 0 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 2.8956 -0.649999 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 2.8956 -1.3 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 2.8956 -1.949999 90) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 1.950001 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.3 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 0.650001 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 0 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at -0.649999 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at -1.3 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at -1.949999 -2.8956) (size 0.381 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 0 0) (size 4.699 4.699) (layers F.Cu F.Paste F.Mask))
)
