(module PIC18F4620-I/P (layer F.Cu)
  (fp_text reference REF** (at 7.62 24.13) (layer F.SilkS))
  (fp_text value PDIP40_600MC_MCH (at 7.62 24.13) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at 18.288 0) (layer Cmts.User))
  (fp_text user "0.6in/15.24mm" (at 7.62 -4.8895) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at 0 53.1495) (layer Cmts.User))
  (fp_text user "*" (at 0.508 0) (layer F.Fab))
  (fp_text user "*" (at 0 -1.5113) (layer F.SilkS))
  (pad 1 thru_hole rect (at 0 0) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 0 17.78) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 20.32) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 22.86) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 25.4) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 27.94) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 30.48) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 33.02) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 0 35.56) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 0 38.1) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 0 40.64) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 0 43.18) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 0 45.72) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 0 48.26) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 15.24 48.26) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 15.24 45.72) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 15.24 43.18) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 15.24 40.64) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 15.24 38.1) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 15.24 35.56) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 15.24 33.02) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 15.24 30.48) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 15.24 27.94) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 15.24 25.4) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 31 thru_hole circle (at 15.24 22.86) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 32 thru_hole circle (at 15.24 20.32) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 33 thru_hole circle (at 15.24 17.78) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 34 thru_hole circle (at 15.24 15.24) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 35 thru_hole circle (at 15.24 12.7) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 36 thru_hole circle (at 15.24 10.16) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 37 thru_hole circle (at 15.24 7.62) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 38 thru_hole circle (at 15.24 5.08) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 39 thru_hole circle (at 15.24 2.54) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 40 thru_hole circle (at 15.24 0) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
)
