(module PIC18F67J94-I/MR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN64_9x9MC_MCH (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -6.4262 -3.5) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at -4.3942 -7.4422) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -7.4422 4.3942) (layer Cmts.User))
  (fp_text user "0.346in/8.788mm" (at 0 9.9822) (layer Cmts.User))
  (fp_text user "0.346in/8.788mm" (at 9.9822 0.635) (layer Cmts.User))
  (fp_text user "0.295in/7.493mm" (at 0 6.7945) (layer Cmts.User))
  (fp_text user "0.295in/7.493mm" (at 6.7945 -0.635) (layer Cmts.User))
  (fp_text user "*" (at -5.4356 -4) (layer F.SilkS))
  (fp_text user "*" (at -3.9878 -4) (layer F.Fab))
  (pad 1 smd rect (at -4.3942 -3.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -4.3942 -3.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -4.3942 -2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -4.3942 -2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -4.3942 -1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -4.3942 -1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -4.3942 -0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -4.3942 -0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -4.3942 0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -4.3942 0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -4.3942 1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -4.3942 1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -4.3942 2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -4.3942 2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -4.3942 3.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -4.3942 3.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -3.75 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -3.250001 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -2.75 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -2.250001 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -1.749999 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at -1.25 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at -0.750001 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at -0.25 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 0.25 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 0.750001 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 1.25 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 1.749999 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 2.250001 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 2.75 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 3.250001 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 3.75 4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 4.3942 3.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 4.3942 3.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 4.3942 2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 4.3942 2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 4.3942 1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 4.3942 1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 4.3942 0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 4.3942 0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at 4.3942 -0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 42 smd rect (at 4.3942 -0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 43 smd rect (at 4.3942 -1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 44 smd rect (at 4.3942 -1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 45 smd rect (at 4.3942 -2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 46 smd rect (at 4.3942 -2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 47 smd rect (at 4.3942 -3.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 48 smd rect (at 4.3942 -3.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 49 smd rect (at 3.75 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 50 smd rect (at 3.250001 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 51 smd rect (at 2.75 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 52 smd rect (at 2.250001 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 53 smd rect (at 1.749999 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 54 smd rect (at 1.25 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 55 smd rect (at 0.750001 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 56 smd rect (at 0.25 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 57 smd rect (at -0.25 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 58 smd rect (at -0.750001 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 59 smd rect (at -1.25 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 60 smd rect (at -1.749999 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 61 smd rect (at -2.250001 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 62 smd rect (at -2.75 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 63 smd rect (at -3.250001 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 64 smd rect (at -3.75 -4.3942) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 65 smd rect (at 0 0) (size 7.493 7.493) (layers F.Cu F.Paste F.Mask))
)
