(module PIC24F16KL402-I/MQ (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN28_5X5MC_MCH (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.508mm" (at -4.4831 -1.27) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at -2.4511 -5.4991) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -5.4991 2.4511) (layer Cmts.User))
  (fp_text user "0.193in/4.902mm" (at 0 8.0391) (layer Cmts.User))
  (fp_text user "0.193in/4.902mm" (at 8.0391 0.635) (layer Cmts.User))
  (fp_text user "0.126in/3.2mm" (at 0 4.6482) (layer Cmts.User))
  (fp_text user "0.126in/3.2mm" (at 4.6482 -0.635) (layer Cmts.User))
  (fp_text user "*" (at -3.4925 -1.778) (layer F.SilkS))
  (fp_text user "*" (at -2.0447 -1.778) (layer F.Fab))
  (pad 1 smd rect (at -2.4511 -1.524 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.4511 -1.016 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.4511 -0.508 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.4511 0 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.4511 0.508 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.4511 1.016 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.4511 1.524 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.524 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.016 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -0.508 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 0 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 0.508 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 1.016 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.524 2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 2.4511 1.524 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 2.4511 1.016 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 2.4511 0.508 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 2.4511 0 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 2.4511 -0.508 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 2.4511 -1.016 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 2.4511 -1.524 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 1.524 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.016 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 0.508 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 0 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at -0.508 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at -1.016 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at -1.524 -2.4511) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 0 0) (size 3.2004 3.2004) (layers F.Cu F.Paste F.Mask))
)
