(module PRG3216P-1072-B-T5 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value RES_3216_SUS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.142in/3.6mm" (at 3.948 0) (layer Cmts.User))
  (fp_text user "0.087in/2.206mm" (at 0 -4.848) (layer Cmts.User))
  (fp_text user "0.028in/0.7mm" (at 0 4.848) (layer Cmts.User))
  (pad 1 smd rect (at -0.7266 0) (size 0.7532 3.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.7266 0) (size 0.7532 3.6) (layers F.Cu F.Paste F.Mask))
)
