(footprint "PWP0028E_N" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "TPA3140D2PWP ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value PWP0028E_N (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "Designator452" (at -3.4036 -6.3246 unlocked) (layer "F.SilkS"))
  (pad "1" smd oval (at -2.799999 -4.225 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd oval (at -2.799999 -3.574999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd oval (at -2.799999 -2.925 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd oval (at -2.799999 -2.274999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd oval (at -2.799999 -1.625001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd oval (at -2.799999 -0.974999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd oval (at -2.799999 -0.325001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd oval (at -2.799999 0.325001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd oval (at -2.799999 0.974999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd oval (at -2.799999 1.625001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd oval (at -2.799999 2.274999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd oval (at -2.799999 2.925 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd oval (at -2.799999 3.574999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd oval (at -2.799999 4.225 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd oval (at 2.799999 4.225 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd oval (at 2.799999 3.574999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd oval (at 2.799999 2.925 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd oval (at 2.799999 2.274999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd oval (at 2.799999 1.625001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd oval (at 2.799999 0.974999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd oval (at 2.799999 0.325001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd oval (at 2.799999 -0.325001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd oval (at 2.799999 -0.974999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd oval (at 2.799999 -1.625001 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd oval (at 2.799999 -2.274999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd oval (at 2.799999 -2.925 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd oval (at 2.799999 -3.574999 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd oval (at 2.799999 -4.225 90) (size 0.349999 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 0 0) (size 2.4 6.170001) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "V" thru_hole circle (at 3E-06 -0.500002) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 1.000001 -0.500002) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 3E-06 0.499999) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 1.000001 0.499999) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 3E-06 1.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 1.000001 1.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 1.000001 -1.500002) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 3E-06 -1.500002) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 1.000001 2.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 3E-06 2.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at -1.000001 2.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at -1.000001 -1.500002) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at -1.000001 1.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at -1.000001 0.499999) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at -1.000001 -0.500002) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at -1.000003 -2.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 0 -2.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 0.999998 -2.5) (size 0.399999 0.399999) (drill 0.2032) (layers *.Cu *.Mask))
)
