(module PinHeader_1x06_P5mm_Vertical (layer F.Cu) (tedit 63229BFB)
  (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x06 2.54mm single row")
  (fp_text reference REF** (at 0 -11.8364) (layer F.SilkS))
  (pad 6 thru_hole oval (at 0 17.399) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 12.3952) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 7.3914) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 2.3876) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 -2.6162) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 -7.62) (size 1.7 1.7) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/1933228--3DModel-STEP-56544.STEP
    (offset (xyz 0 7.62 1.143))
    (scale (xyz 1 1 1))
    (rotate (xyz 90 0 90))
  )
)
