(module PinSocket_1x06_P1.00mm_Vertical (layer F.Cu) (tedit 5A19A41C)
  (descr "Through hole straight socket strip, 1x06, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated")
  (tags "Through hole socket strip THT 1x06 1.00mm single row")
  (fp_text reference REF** (at -0.29 -2.25) (layer F.SilkS))
  (fp_text value PinSocket_1x06_P1.00mm_Vertical (at -0.29 7.25) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 1) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 2) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 3) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 4) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0 5) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
  (fp_text user %R (at -0.29 2.5 90) (layer F.Fab))
  (model ${KISYS3DMOD}/Connector_PinSocket_1.00mm.3dshapes/PinSocket_1x06_P1.00mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)