(module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right (layer F.Cu) (tedit 635C0422)
  (descr "surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated")
  (tags "Surface mounted socket strip SMD 1x08 2.54mm single row style2 pin1 right")
  (attr smd)
  (fp_text reference REF** (at 0 -11.76) (layer F.SilkS))
  (pad 7 smd rect (at 1.65 6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.65 1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.65 -3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 1.65 -8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.65 8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.65 3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.65 -1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.65 -6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
