(module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm (layer F.Cu) (tedit 61FD4BC4)
  (descr "QFN, 16 Pin (http://cds.linear.com/docs/en/datasheet/37551fd.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.82) (layer F.SilkS))
  (fp_text value QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm (at 0 2.82) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd roundrect (at 0.36 0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.36 -0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.36 0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.36 -0.36) (size 0.58 0.58) (layers F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd rect (at 0 0) (size 1.45 1.45) (layers F.Cu F.Mask))
  (pad 16 smd rect (at -0.75 -1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -0.25 -1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 0.25 -1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0.75 -1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.75 1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.25 1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -0.25 1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.75 1.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
