(module Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm (layer F.Cu) (tedit 61D48F09)
  (descr "QFN, 16 Pin (http://www.thatcorp.com/datashts/THAT_1580_Datasheet.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -3.32) (layer F.SilkS))
  (fp_text value QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm (at 0 3.32) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd roundrect (at 0.525 0.525) (size 0.85 0.85) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.525 -0.525) (size 0.85 0.85) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.525 0.525) (size 0.85 0.85) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.525 -0.525) (size 0.85 0.85) (layers F.Paste) (roundrect_rratio 0.25))
  (pad 17 smd rect (at 0 0) (size 2.1 2.1) (layers F.Cu F.Mask))
  (pad 16 smd rect (at -0.975 -1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -0.325 -1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 0.325 -1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0.975 -1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 1.95 -0.975) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.95 -0.325) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.95 0.325) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.95 0.975) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.975 1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.325 1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -0.325 1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.975 1.95) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.95 0.975) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.95 0.325) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.95 -0.325) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.95 -0.975) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
