(module QFN-24-EP (layer F.Cu) (tedit 6478BCEC)
  (descr "<h3>24-Pin QFN w/ Center Pad (4 x 4 mm)</h3><p><a href=\"http://cdn.sparkfun.com/datasheets/Components/General%20IC/PS-MPU-6000A.pdf\">Datasheet</a></p><p>Specifications:<ul><li>Pin Count: 24</li><li>Area: 4.0 x 4.0 x 0.90 mm</li><li>Pitch: 0.5 mm</li></ul><p>Devices Using:</p><ul><li>MPU-6000</li></ul>")
  (attr smd)
  (fp_text reference REF** (at 0 -3.0988) (layer F.SilkS))
  (fp_text value MPU-6000 (at 0 3.0988) (layer F.Fab))
  (fp_text user Y (at -0.6 -1) (layer F.Fab))
  (fp_text user X (at 1.1 -0.4) (layer F.Fab))
  (fp_text user Z (at -0.1 0.6) (layer F.Fab))
  (pad 1 smd oval (at -2.0662 -1.2567 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -2.0662 -0.7496 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -2.0662 -0.2475 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -2.0662 0.2875 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -2.0662 0.7921 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -2.0662 1.2967 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at -1.2667 2.1216 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at -0.7621 2.1216 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at -0.2575 2.1216 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 0.2775 2.1216 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 0.7796 2.1216 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 1.2867 2.1216 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 2.0862 1.2967 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 2.0862 0.7921 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at 2.0862 0.2875 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at 2.0862 -0.2475 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at 2.0862 -0.7496 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at 2.0862 -1.2567 180) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at 1.2867 -2.0816 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at 0.7796 -2.0816 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd oval (at 0.2775 -2.0816 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd oval (at -0.2575 -2.0816 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd oval (at -0.7621 -2.0816 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd oval (at -1.2667 -2.0816 90) (size 1.016 0.254) (layers F.Cu F.Paste F.Mask))
  (pad P$1 smd rect (at 0.02 0.01) (size 2.6162 2.6162) (layers F.Cu F.Mask))
)
