(module QFN-28_4x4mm_P0.5mm (layer F.Cu) (tedit 5D9F792A)
  (descr "QFN, 28 Pin (http://www.st.com/resource/en/datasheet/stm32f031k6.pdf#page=90), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -3.32) (layer F.SilkS))
  (fp_text value QFN-28_4x4mm_P0.5mm (at 0 3.32) (layer F.Fab))
  (pad 1 smd custom (at -1.9975 -1.5) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.3325 -0.08) (xy 0.19886 -0.08) (xy 0.3325 0.05364) (xy 0.3325 0.08)
         (xy -0.3325 0.08)) (width 0.09))
    ))
  (pad 2 smd rect (at -1.9375 -1) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -1.9375 -0.5) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -1.9375 0) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at -1.9375 0.5) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at -1.9375 1) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd custom (at -1.9975 1.5) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.3325 -0.08) (xy 0.3325 -0.08) (xy 0.3325 -0.05364) (xy 0.19886 0.08)
         (xy -0.3325 0.08)) (width 0.09))
    ))
  (pad 8 smd custom (at -1.5 1.9975) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.08 -0.19886) (xy 0.05364 -0.3325) (xy 0.08 -0.3325) (xy 0.08 0.3325)
         (xy -0.08 0.3325)) (width 0.09))
    ))
  (pad 9 smd rect (at -1 1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd rect (at -0.5 1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd rect (at 0 1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd rect (at 0.5 1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd rect (at 1 1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd custom (at 1.5 1.9975) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.08 -0.3325) (xy -0.05364 -0.3325) (xy 0.08 -0.19886) (xy 0.08 0.3325)
         (xy -0.08 0.3325)) (width 0.09))
    ))
  (pad 15 smd custom (at 1.9975 1.5) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.3325 -0.08) (xy 0.3325 -0.08) (xy 0.3325 0.08) (xy -0.19886 0.08)
         (xy -0.3325 -0.05364)) (width 0.09))
    ))
  (pad 16 smd rect (at 1.9375 1) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 17 smd rect (at 1.9375 0.5) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 18 smd rect (at 1.9375 0) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 19 smd rect (at 1.9375 -0.5) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 20 smd rect (at 1.9375 -1) (size 0.875 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 21 smd custom (at 1.9975 -1.5) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.3325 0.05364) (xy -0.19886 -0.08) (xy 0.3325 -0.08) (xy 0.3325 0.08)
         (xy -0.3325 0.08)) (width 0.09))
    ))
  (pad 22 smd custom (at 1.5 -1.9975) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.08 -0.3325) (xy 0.08 -0.3325) (xy 0.08 0.19886) (xy -0.05364 0.3325)
         (xy -0.08 0.3325)) (width 0.09))
    ))
  (pad 23 smd rect (at 1 -1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 24 smd rect (at 0.5 -1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 25 smd rect (at 0 -1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 26 smd rect (at -0.5 -1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 27 smd rect (at -1 -1.9375) (size 0.25 0.875) (layers F.Cu F.Mask F.Paste))
  (pad 28 smd custom (at -1.5 -1.9975) (size 0.136863 0.136863) (layers F.Cu F.Mask F.Paste)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy -0.08 -0.3325) (xy 0.08 -0.3325) (xy 0.08 0.3325) (xy 0.05364 0.3325)
         (xy -0.08 0.19886)) (width 0.09))
    ))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28_4x4mm_P0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)