(footprint "RASPI_ZERO_FULL"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Raspberry Pi board model B+, full outline with position of big connectors &amp; drill holes")
	(property "Reference" "Ref**"
		(at 32.9 -14.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Val**"
		(at 32.9 -11.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "GND"
		(at 11.9 -2.8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "D-"
		(at 25.8 -1.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "+5V"
		(at 12.2 -5.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "D+"
		(at 19.9 -1.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "" np_thru_hole circle
		(at 3.5 -26.5)
		(size 2.75 2.75)
		(drill 2.75)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.5 -3.5)
		(size 2.75 2.75)
		(drill 2.75)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 61.5 -26.5)
		(size 2.75 2.75)
		(drill 2.75)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 61.5 -3.5)
		(size 2.75 2.75)
		(drill 2.75)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 56.63 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "2" thru_hole circle
		(at 56.63 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "3" thru_hole circle
		(at 54.09 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "4" thru_hole circle
		(at 54.09 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "5" thru_hole circle
		(at 51.55 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "6" thru_hole circle
		(at 51.55 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "7" thru_hole circle
		(at 49.01 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "8" thru_hole circle
		(at 49.01 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "9" thru_hole circle
		(at 46.47 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "10" thru_hole circle
		(at 46.47 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "11" thru_hole circle
		(at 43.93 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "12" thru_hole circle
		(at 43.93 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "13" thru_hole circle
		(at 41.39 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "14" thru_hole circle
		(at 41.39 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "15" thru_hole circle
		(at 38.85 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "16" thru_hole circle
		(at 38.85 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "17" thru_hole circle
		(at 36.31 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "18" thru_hole circle
		(at 36.31 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "19" thru_hole circle
		(at 33.77 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "20" thru_hole circle
		(at 33.77 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "21" thru_hole circle
		(at 31.23 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "22" thru_hole circle
		(at 31.23 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "23" thru_hole circle
		(at 28.69 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "24" thru_hole circle
		(at 28.69 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "25" thru_hole circle
		(at 26.15 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "26" thru_hole circle
		(at 26.15 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "27" thru_hole circle
		(at 23.61 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "28" thru_hole circle
		(at 23.61 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "29" thru_hole circle
		(at 21.07 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "30" thru_hole circle
		(at 21.07 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "31" thru_hole circle
		(at 18.53 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "32" thru_hole circle
		(at 18.53 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "33" thru_hole circle
		(at 15.99 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "34" thru_hole circle
		(at 15.99 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "35" thru_hole circle
		(at 13.45 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "36" thru_hole circle
		(at 13.45 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "37" thru_hole circle
		(at 10.91 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "38" thru_hole circle
		(at 10.91 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "39" thru_hole circle
		(at 8.37 -25.23)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "40" thru_hole circle
		(at 8.37 -27.77)
		(size 1.778 1.778)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "PP1" thru_hole circle
		(at 11.2 -6.3)
		(size 1.7 1.7)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "PP6" thru_hole circle
		(at 10.9 -3.5)
		(size 1.7 1.7)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "PP22" thru_hole circle
		(at 23 -1.85)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "PP23" thru_hole circle
		(at 24.85 -1.85)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu" "*.Mask" "B.Fab")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 6.6 -3.5) (xy 6.580508 -3.84709) (xy 6.522277 -4.189815) (xy 6.426038 -4.523865) (xy 6.293003 -4.84504)
				(xy 6.124845 -5.149299) (xy 5.923678 -5.432818) (xy 5.692031 -5.692031) (xy 5.432818 -5.923678)
				(xy 5.149299 -6.124845) (xy 4.84504 -6.293003) (xy 4.523865 -6.426038) (xy 4.189815 -6.522277) (xy 3.84709 -6.580508)
				(xy 3.5 -6.6) (xy 3.15291 -6.580508) (xy 2.810185 -6.522277) (xy 2.476135 -6.426038) (xy 2.15496 -6.293003)
				(xy 1.850701 -6.124845) (xy 1.567182 -5.923678) (xy 1.307969 -5.692031) (xy 1.076322 -5.432818)
				(xy 0.875155 -5.149299) (xy 0.706997 -4.84504) (xy 0.573962 -4.523865) (xy 0.477723 -4.189815) (xy 0.419492 -3.84709)
				(xy 0.4 -3.5) (xy 0.419492 -3.15291) (xy 0.477723 -2.810185) (xy 0.573962 -2.476135) (xy 0.706997 -2.15496)
				(xy 0.875155 -1.850701) (xy 1.076322 -1.567182) (xy 1.307969 -1.307969) (xy 1.567182 -1.076322)
				(xy 1.850701 -0.875155) (xy 2.15496 -0.706997) (xy 2.476135 -0.573962) (xy 2.810185 -0.477723) (xy 3.15291 -0.419492)
				(xy 3.5 -0.4) (xy 3.84709 -0.419492) (xy 4.189815 -0.477723) (xy 4.523865 -0.573962) (xy 4.84504 -0.706997)
				(xy 5.149299 -0.875155) (xy 5.432818 -1.076322) (xy 5.692031 -1.307969) (xy 5.923678 -1.567182)
				(xy 6.124845 -1.850701) (xy 6.293003 -2.15496) (xy 6.426038 -2.476135) (xy 6.522277 -2.810185) (xy 6.580508 -3.15291)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu" "*.Mask" "B.Fab")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64.6 -26.5) (xy 64.580508 -26.84709) (xy 64.522277 -27.189815) (xy 64.426038 -27.523865) (xy 64.293003 -27.84504)
				(xy 64.124845 -28.149299) (xy 63.923678 -28.432818) (xy 63.692031 -28.692031) (xy 63.432818 -28.923678)
				(xy 63.149299 -29.124845) (xy 62.84504 -29.293003) (xy 62.523865 -29.426038) (xy 62.189815 -29.522277)
				(xy 61.84709 -29.580508) (xy 61.5 -29.6) (xy 61.15291 -29.580508) (xy 60.810185 -29.522277) (xy 60.476135 -29.426038)
				(xy 60.15496 -29.293003) (xy 59.850701 -29.124845) (xy 59.567182 -28.923678) (xy 59.307969 -28.692031)
				(xy 59.076322 -28.432818) (xy 58.875155 -28.149299) (xy 58.706997 -27.84504) (xy 58.573962 -27.523865)
				(xy 58.477723 -27.189815) (xy 58.419492 -26.84709) (xy 58.4 -26.5) (xy 58.419492 -26.15291) (xy 58.477723 -25.810185)
				(xy 58.573962 -25.476135) (xy 58.706997 -25.15496) (xy 58.875155 -24.850701) (xy 59.076322 -24.567182)
				(xy 59.307969 -24.307969) (xy 59.567182 -24.076322) (xy 59.850701 -23.875155) (xy 60.15496 -23.706997)
				(xy 60.476135 -23.573962) (xy 60.810185 -23.477723) (xy 61.15291 -23.419492) (xy 61.5 -23.4) (xy 61.84709 -23.419492)
				(xy 62.189815 -23.477723) (xy 62.523865 -23.573962) (xy 62.84504 -23.706997) (xy 63.149299 -23.875155)
				(xy 63.432818 -24.076322) (xy 63.692031 -24.307969) (xy 63.923678 -24.567182) (xy 64.124845 -24.850701)
				(xy 64.293003 -25.15496) (xy 64.426038 -25.476135) (xy 64.522277 -25.810185) (xy 64.580508 -26.15291)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu" "*.Mask" "B.Fab")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64.6 -3.5) (xy 64.580508 -3.84709) (xy 64.522277 -4.189815) (xy 64.426038 -4.523865) (xy 64.293003 -4.84504)
				(xy 64.124845 -5.149299) (xy 63.923678 -5.432818) (xy 63.692031 -5.692031) (xy 63.432818 -5.923678)
				(xy 63.149299 -6.124845) (xy 62.84504 -6.293003) (xy 62.523865 -6.426038) (xy 62.189815 -6.522277)
				(xy 61.84709 -6.580508) (xy 61.5 -6.6) (xy 61.15291 -6.580508) (xy 60.810185 -6.522277) (xy 60.476135 -6.426038)
				(xy 60.15496 -6.293003) (xy 59.850701 -6.124845) (xy 59.567182 -5.923678) (xy 59.307969 -5.692031)
				(xy 59.076322 -5.432818) (xy 58.875155 -5.149299) (xy 58.706997 -4.84504) (xy 58.573962 -4.523865)
				(xy 58.477723 -4.189815) (xy 58.419492 -3.84709) (xy 58.4 -3.5) (xy 58.419492 -3.15291) (xy 58.477723 -2.810185)
				(xy 58.573962 -2.476135) (xy 58.706997 -2.15496) (xy 58.875155 -1.850701) (xy 59.076322 -1.567182)
				(xy 59.307969 -1.307969) (xy 59.567182 -1.076322) (xy 59.850701 -0.875155) (xy 60.15496 -0.706997)
				(xy 60.476135 -0.573962) (xy 60.810185 -0.477723) (xy 61.15291 -0.419492) (xy 61.5 -0.4) (xy 61.84709 -0.419492)
				(xy 62.189815 -0.477723) (xy 62.523865 -0.573962) (xy 62.84504 -0.706997) (xy 63.149299 -0.875155)
				(xy 63.432818 -1.076322) (xy 63.692031 -1.307969) (xy 63.923678 -1.567182) (xy 64.124845 -1.850701)
				(xy 64.293003 -2.15496) (xy 64.426038 -2.476135) (xy 64.522277 -2.810185) (xy 64.580508 -3.15291)
			)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/Raspberry_Pi_Zero_V1.3.STEP"
		(offset
			(xyz 65 0 -11.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 180 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/CPG-01-TH-B.STEP"
		(offset
			(xyz 10.9 3.5 0.3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/CPG-01-TH-B.STEP"
		(offset
			(xyz 11.2 6.3 0.3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/CPG-01-TH-B.STEP"
		(offset
			(xyz 23 1.85 0.3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/CPG-01-TH-B.STEP"
		(offset
			(xyz 24.85 1.85 0.3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.step"
		(offset
			(xyz 8.37 27.77 -1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 0 90)
		)
	)
	(model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.step"
		(offset
			(xyz 8.37 27.77 -11.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/970100155.stp"
		(offset
			(xyz 3.5 3.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/970100155.stp"
		(offset
			(xyz 3.5 26.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/970100155.stp"
		(offset
			(xyz 61.5 3.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/970100155.stp"
		(offset
			(xyz 61.5 26.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 3.5 3.5 -6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 3.5 26.5 -6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 61.5 3.5 -6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 61.5 26.5 -6)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 3.5 3.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 3.5 26.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 61.5 3.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
	(model "C:/Users/vasil/Documents/GitHub/raspi-zero-full-kicad/Raspberry_Pi_Zero_v.1.3_Hat.pretty/29331.STEP"
		(offset
			(xyz 61.5 26.5 -6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)