(footprint "RC1206N_VIS" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "WSL1206R1500FEA ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value RC1206N_VIS (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.799198 -0.749198)
        (xy 0.799198 -0.749198)
        (xy 0.799198 0.749198)
        (xy -0.799198 0.749198)
      )
    )
  )
  (pad "1" smd rect (at -1.402798 0) (size 1.105598 1.599997) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 1.402798 0) (size 1.105598 1.599997) (layers "F.Cu" "F.Paste" "F.Mask"))
)
